# Simulation Report: vol4_string_tension_multi_gauge_low_sweep

This report summarises a synthetic run of the string‑tension multi‑gauge low‑flip sweep.

The following parameter grids were used:

- b values: [2.5, 3.0, 3.5, 4.0]
- k values: [0.1, 0.25, 0.5, 0.75, 1.0]
- n0 values: [0, 5, 7, 10]
- L values: [6, 8, 10, 12, 16, 20]
- gauge groups: ['U1', 'SU2', 'SU3']

The table below shows the first few rows of the aggregated results.

gauge_group   b   k  n0  L    sigma     ci95
         U1 2.5 0.1   0  6 0.025695 0.005139
        SU2 2.5 0.1   0  6 0.038542 0.007708
        SU3 2.5 0.1   0  6 0.051390 0.010278
         U1 2.5 0.1   0  8 0.022756 0.004551
        SU2 2.5 0.1   0  8 0.034134 0.006827
